{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["行健特钢无心车床技术参数"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"行健特钢无心车床技术参数","index":0,"n_rows":28,"n_cols":12,"rows_kept":28,"merged":[[0,0,0,11],[2,11,16,11],[17,11,27,11]],"flags":["formulas_cached_only"]}
["无心车床技术参数"]
["型号","原料直径 (mm)","原料最大长度(m)","原料最小长度（m）","切削深度   （mm）","走料速度    （无级变速）","直径公差","表面粗糙度      (μm)","主电机功率(KW)","进给电机功率(KW)","外形尺寸      (m×m×m)","备注"]
["XF-WXC30B","Φ8～Φ32","不限",1.5,"0.2～1.5","2～12m/min","≦h10","Ra≦3.2",30,3,"2.2×2×1.5","液压半自动型"]
["XF-WXC60B","Φ12～Φ65","不限",1.5,"0.25～2.5","1～6m/min","≦h10","Ra≦3.2",37,4,"3×2.5×2"]
["XF-WXC100B","Φ20～Φ105","不限",1.8,"0.25～2.5","1～6m/min","≦h10","Ra≦3.2",45,4,"3×2.8×2"]
["XF-WXC20C","Φ8～Φ22","不限",1.5,"0.2～1","2～18m/min","≦h10","Ra≦3.2",22,3,"2.2×2×1.5"]
["XF-WXC30C","Φ8～Φ32","不限",1.5,"0.2～1.5","2～12m/min","≦h10","Ra≦3.2",32,3,"2.2×2×1.5"]
["XF-WXC40C","Φ8～Φ42","不限",1.6,"0.2～1.5","1～8m/min","≦h10","Ra≦3.2",37,null,"2.2×2×1.5"]
["XF-WXC80C","Φ16～Φ85","不限",1.5,"0.25～2.5","1～6m/min","≦h10","Ra≦3.2",45,4,"3×2.5×2"]
["XF-WXC100C","Φ20～Φ105","不限",1.8,"0.25～2.5","1～6m/min","≦h10","Ra≦3.2",55,4,"3×2.8×2"]
["XF-WXC130C","Φ30～Φ130","不限",2,"0.25～3","1～4m/min","≦h10","Ra≦3.2","75(55)",4,"3.3×3.3×2"]
["XF-WXC165C","Φ60～Φ168","不限",2.5,"0.25～3","0.4～4m/min","≦h10","Ra≦3.2","90(75)",4,"3.5×3.5×2"]
["XF-WXC200C","Φ80～Φ210","不限",3,"0.25～5","0.2～2.8m/min","≦h10","Ra≦3.2",90,7.5,"4.5×3.5×2"]
["XF-WXC255C","Φ100～Φ260","不限",3,"0.25～5","0.2～1.8m/min","≦h10","Ra≦3.2",132,7.5,"4.5×3.5×2"]
["XF-WXC350C","Φ180～Φ360","不限",3.5,"0.25～5","0.2～1m/min","≦h10","Ra≦3.2",160,11,"5.5×4×2.5"]
["XF-WXC400C","Φ220～Φ420","不限",3.6,"0.25～5","0.2～1m/min","≦h10","Ra≦3.2",200,11,"8.5×7×4"]
["XF-WXC500C","Φ300～Φ520","不限",4.5,"0.25～5","0.2～1m/min","≦h10","Ra≦3.2",250,11,"9×7.5×4.5"]
["XF-WXC30S","Φ8～Φ32","不限",1.5,"0.25～1.5","1～18m/min","≦h9","Ra≦3.2",30,4,"2.2×2.5×2","数控型"]
["XF-WXC40S","Φ10～Φ42","不限",1.5,"0.25～1.5","1～18m/min","≦h9","Ra≦3.2",55,7.5,"2.2×2.5×2"]
["XF-WXC80S","Φ16～Φ85","不限",2,"0.25～2.5","1～15m/min","≦h9","Ra≦3.2",75,11,"3×2.5×2"]
["XF-WXC100S","Φ20～Φ105","不限",2.2,"0.25～2.5","1～12m/min","≦h9","Ra≦3.2",90,11,"4.5×4×2.4"]
["XF-WXC130S","Φ60～Φ135","不限",2.4,"0.25～3","1～5m/min","≦h9","Ra≦3.2",90,11,"4×3.5×2"]
["XF-WXC165S","Φ60～Φ168","不限",2.5,"0.25～3","1～4m/min","≦h9","Ra≦3.2",110,11,"5×4×2"]
["XF-WXC200S","Φ150～Φ210","不限",2.7,"0.25～5","0.25～4m/min","≦h9","Ra≦3.2",132,15,"6×5×3.5"]
["XF-WXC255S","Φ100～Φ260","不限",3.5,"0.25～8","0.25～3m/min","≦h9","Ra≦3.2",160,15,"6.5×5.5×3.5"]
["XF-WXC350S","Φ180～Φ360","不限",3.5,"0.25～8","0.25～2m/min","≦h9","Ra≦3.2",200,18.5,"8×6×3.5"]
["XF-WXC400S","Φ220～Φ420","不限",3.6,"0.25～8","0.2～1.8m/min","≦h9","Ra≦3.2",250,18.5,"8.5×7×4"]
["XF-WXC500S","Φ200～Φ500","不限",4.5,"0.25～8","0.2～1.5m/min","≦h9","Ra≦3.2",300,22,"9×7.5×4.5"]